|  |  |  |  |
| --- | --- | --- | --- |
| How to Guide – BANNED ITEMS & PRACTICES | | | |
| What: | To outline the Banned Items and Practices from Operations and sites. | | |
| When: | Operations on Oil and Gas Sites. | | |
| Why: | An integrated Industry ban on identified risks which pose unacceptable risk to users and operations | | |
| Who: | All Personnel working on Australian Onshore Oil and Gas Sites. | | |
| How: | Ensure the following items are not taken to site or if found at site, reported and removed as soon as practicable. Banned practices should not be carried out. | | |
| 9” Angle Grinder |  | https://tse4.mm.bing.net/th?id=OIP.tVq3HSQ_6O454zYZycP86AHaEJ&pid=ApiHome-made & Non-engineered Tools |
| Minsup clips, R-clips, Diaper Pins & any other type of safety pins that can fail to open | | |
| Octopus Straps |  | https://tse3.mm.bing.net/th?id=OIP.6XO7LF8JOZRHJYD2Z1Ko0wHaHa&pid=ApiSingle-Action Load Binders |
| For Lifting Operations, all shackles must be certified 4-piece shackles.  3-piece allowable for all other activities. |  | https://tse2.mm.bing.net/th?id=OIP.KnvB3nqe7eKrpJYor5JzZQHaHa&pid=Apihttps://tse1.mm.bing.net/th?id=OIP.RHW6P55J30FK-cOWV0U_2wHaHa&pid=ApiNon-Auto Retracting Blades |
| Banned Practice #1: (WIS) During E-Line operations, do not use the UHF inside the Wireline Unit whilst winch is moving / operating. | | |